Amcrest IPM-HX1b
(TenFourFox Needed)

View Extra Stream
rtsp://admin:ROGH6360amcrest@192.168.1.138:554/cam/realmonitor?channel=1&subtype=1

View Main Stream
rtsp://admin:ROGH6360amcrest@192.168.1.138:554/cam/realmonitor?channel=1&subtype=0

Create  Finder 
http://192.168.1.138/cgi-bin/mediaFileFind.cgi?action=factory.create

Files satisfied the conditions with the Finder 
http://192.168.1.138/cgi-bin/mediaFileFind.cgi?action=findFile&object=2086170840&condition.Chann 
el=1&condition.Dirs[0]=/mnt/dvr/sda0&condition.Types[0]=dav&condition.Events[0]=AlarmLocal&con 
dition.Events[1]=VideoMotion&condition.StartTime=2019-1-1%2019:00:00&condition.EndTime= 2020- 
1-10% 2020:00:00&condition.VideoStream=Main 

Get the media file info found by finder
http://192.168.1.138/cgi-bin/mediaFileFind.cgi?action=findNextFile&object=XXXXX&count=100 

Download media file with file name 
http://192.168.1.138/cgi-bin/RPC_Loadfile/mnt/sd/2015-01-08/001/dav/19/19.57.12-19.58.25[M][0@0] [0].dav 

Download media file between times
http://192.168.1.108/cgi-bin/loadfile.cgi?action=startLoad&channel=1&startTime=2019-10-8%2020:00 
:01&endTime=2019-10-8%2020:00:01&subtype=0 

Close Finder 
http://192.168.1.138/cgi-bin/mediaFileFind.cgi?action=close&object=XXXXX

Destroy Finder 
http://192.168.1.138/cgi-bin/mediaFileFind.cgi?action=destroy&object=XXXXX

Serial Number
http://192.168.1.138/cgi-bin/magicBox.cgi?action=getSerialNo

sn=AMC016R77E4R4GQ29B

System Info
http://192.168.1.138/cgi-bin/magicBox.cgi?action=getSystemInfo

appAutoStart=true
deviceType=IPM-HX1B
hardwareVersion=1.00
processor=S2LM
serialNumber=AMC016R77E4R4GQ29B
updateSerial=IPC-C15-Amcrest
updateSerialCloudUpgrade=IPC-C15-Amcrest:01:02:0F:38:16:00:01:0F:01:01:04:258:00:02:00:00:00:00:00:00:100

Onvif Version
http://192.168.1.138/cgi-bin/IntervideoManager.cgi?action=getVersion&Name=Onvif

version=16.12(V2.4.1.513183)

Back Up Config
http://192.168.1.138/cgi-bin/Config.backup?action=All 

Restore Config
http://192.168.1.138/cgi-bin/configManager.cgi?action=restore&names[0]=<xxx>&names[1]=<yyy>[&…] 

xxx and yyy is config name which need to be restore

Reboot Device
http://192.168.1.138/cgi-bin/magicBox.cgi?action=reboot[&delay=<0>]